L20 Doors/ shutters/ hatches
	To be read with Preliminaries/ General conditions.
	GENERAL
	110	EVIDENCE OF PERFORMANCE
	•	 Certification: Provide independently certified evidence that all incorporated components 
	comply with specified performance requirements. As per Architects Drawing
	120	NON FIRE RESISTING DOORS/ DOORSETS/ ASSEMBLIES
	•	 Provide certified evidence, in the form of a product conformity certificate or engineering 
	assessment, that each door/ doorset/ assembly supplied will comply with the specified 
	requirements to BS EN 14351-1. Such certification must cover door and frame materials, 
	glass and glazing materials and their installation, essential and ancillary ironmongery, 
	hinges and seals. 
	150	SITE DIMENSIONS
	•	 Procedure: Before starting work on designated items take site dimensions, record on shop 
	drawings and use to ensure accurate fabrication. 
	•	 Designated items: 
	Doors . 
	PRODUCTS
	460	FRAMELESS GLASS DOORS As Per Architects Drawings
	•	 Manufacturer: Comar Architectural Aluminium Systems. The Parkside Group Ltd. 
	Unit 5 The Willow Centre17 Willow Lane Mitcham Surrey CR4 4NX.Tel:020 8685 
	9685. 
	Fax: 020 8646 5096. Email: Projects@Parksidegroup.co.uk Web: www.comar-
	alu.co.uk . . 
	-	Product reference: Comar 7 AG Doors Kitemark License Number KM593756-BS 
  
	•	 Door leaf: Safety glass to BS EN 12600, class ________. 
	-	Thickness: ________. 
	-	Colour: ________. 
	•	 Decoration: ________. 
	-	Manifestation: ________. 
	•	 Door rails/ Patch fittings: ________. 
	-	Material/ Finish: ________. 
	•	 Peripheral fixings: ________. 
	•	 Lock: ________. 
	-	Position: ________. 
	•	 Floor springs: ________. 
	•	 Pull handles: ________. 
	-	Size: ________. 
	-	Material/ Finish: ________. 
	•	 Additional ironmongery/ accessories: ________. 

	480	DOORSETS ALUMINIUM As Per Architects Drawings
	•	 Manufacturer: Comar Architectural Aluminium Systems. The Parkside Group Ltd. 
	Unit 5 The Willow Centre17 Willow Lane Mitcham Surrey CR4 4NX.Tel:020 8685 
	9685. 
	Fax: 020 8646 5096. Email: Projects@Parksidegroup.co.uk Web: www.comar-
	alu.co.uk . . 
	-	Product reference: Comar ???? Kitemark License Number KM593756-BS 
	
Comar 7Pi Commercial Door
Comar 9Pi High Performance Rebated Door
Comar 7 AG Doors
Comar 7 Aluminium Doorsets
Comar 7Pi ECO Insulated Doors
Comar 7P.i Folding Sliding Door
Comar 7 P i High Performance Doors
Comar 7 P i HSD Horizontal Sliding Door System
Comar 7 Tempest High Performance Doors ???
	4873/PAS24:2012 , Secured by Design License Holder .  

	•	 Door leaf: Extruded aluminium profiles of aluminium alloy 6063 T5, T6 to BS EN 755-1: 
	2008. . 
	-	Finish as delivered: _______ . 
	•	 Frame and architraves: Extruded aluminium profiles of aluminium alloy 6063 T5, T6 to BS 
	EN 755-1: 2008. . 
	-	Finish as delivered: ________ . 
	•	 Glazing details: _______ . 
	-	Beading: ________ . 
	•	 Ironmongery: _______ . 
	•	 Perimeter seals: _______ . 
	•	 Other requirements: ________ . 
	•	 Fixing: As per Comar Tecnical Manual . 
	490	AUTOMATIC DOORS ALUMINIUM As Per Architects Drawings
	•	 Type: ________. 
	•	 Manufacturer: Comar Architectural Aluminium Systems. The Parkside Group Ltd. 
	Unit 5 The Willow Centre17 Willow Lane Mitcham Surrey CR4 4NX.Tel:020 8685 
	9685. 
	Fax: 020 8646 5096. Email: Projects@Parksidegroup.co.uk Web: www.comar-
	alu.co.uk . 
	-	Product reference: Comar 7 Doors . 
	•	 Materials/ finishes: 
	-	Doors: Extruded aluminium profiles of aluminium alloy 6063 T5, T6 to BS EN 755-1: 
	2008. . 
	-	Frames: Extruded aluminium profiles of aluminium alloy 6063 T5, T6 to BS EN 755-1: 
	2008. . 
	-	Screens: ________ . 
	•	 Glazing/ Infill details: ________ . 
	-	Manifestation: ________ . 
	•	 Activation and control system: ________ . 
	-	Safety devices: ________ . 
	-	Breakout facility: ________ . 
	•	 Locking mechanism: ________ . 
	•	 Signs: ________ . 
	•	 Barriers: ________ . 
	•	 Other requirements: ________ . 

	520	SLIDING DOORSALUMINIUM As Per Architects Drawings
	•	 Manufacturer: Comar Architectural Aluminium Systems. The Parkside Group Ltd. 
	Unit 5 The Willow Centre17 Willow Lane Mitcham Surrey CR4 4NX.Tel:020 8685 
	9685. 
	Fax: 020 8646 5096. Email: Projects@Parksidegroup.co.uk Web: www.comar-
	alu.co.uk . 
	-	Product reference: Comar 7 or Comar 7Pi sliding Doors . 
	•	 Performance: ________ . 
	•	 Arrangement: ________ . 
	-	Track system: ________ . 
	•	 Door leaf: Extruded aluminium profiles of aluminium alloy 6063 T5, T6 to BS EN 755-1: 
	2008 . 
	-	Finish as delivered: ________ . 
	-	Glazing/ Infill details: ________ . 
	Manifestation: ________ . 
	•	 Operation: Manual . 
	•	 Ironmongery: ________ . 
	•	 Other requirements: ________ . 
	525	SLIDING POCKET DOORSALUMINIUM As Per Architects Drawings
	•	 Manufacturer: Comar Architectural Aluminium Systems. The Parkside Group Ltd. 
	Unit 5 The Willow Centre17 Willow Lane Mitcham Surrey CR4 4NX.Tel:020 8685 
	9685. 
	Fax: 020 8646 5096. Email: Projects@Parksidegroup.co.uk Web: www.comar-
	alu.co.uk . 
	-	Product reference: Comar 7 or Comar 7Pi sliding Doors . 
	•	 Performance: ________ . 
	•	 Arrangement: ________ . 
	-	Track system: ________ . 
	•	 Door leaf: Extruded aluminium profiles of aluminium alloy 6063 T5, T6 to BS EN 755-1: 
	2008 . 
	-	Finish as delivered: ________ . 
	-	Glazing/ Infill details: ________ . 
	Manifestation: ________ . 
	•	 Operation: Manual . 
	•	 Ironmongery: ________ . 
	•	 Other requirements: ________ . 
	530	SLIDING FOLDING EXTERNAL DOORSALUMINIUM As Per Architects Drawings
	•	 Manufacturer: Comar Architectural Aluminium Systems. The Parkside Group Ltd. 
	Unit 5 The Willow Centre17 Willow Lane Mitcham Surrey CR4 4NX.Tel:020 8685 
	9685. 
	Fax: 020 8646 5096. Email: Projects@Parksidegroup.co.uk Web: www.comar-
	alu.co.uk . 
	-	Product reference: Comar 7Pi FSD . 
	•	 Performance: ________ . 
	•	 Arrangement: ________ . 
	-	Track system: ________ . 
	•	 Door leaf: Extruded aluminium profiles of aluminium alloy 6063 T5, T6 to BS EN 755-1: 
	2008 . 
	-	Finish as delivered: ________ . 
	-	Glazing/ Infill details: ________ . 
	Manifestation: ________ . 
	•	 Operation: Manual . 
	•	 Ironmongery: ________ . 
	•	 Other requirements: ________ . 

	EXECUTION
	710	PROTECTION OF COMPONENTS
	•	 General: Do not deliver to site components that cannot be installed immediately or placed 
	in clean, dry, floored and covered storage. 
	•	 Stored components: Stacked on level bearers, separated with spacers to prevent damage 
	by and to projecting ironmongery, beads, etc. 
	830	FIXING IRONMONGERY GENERALLY
	•	 Fasteners: Supplied by ironmongery manufacturer. 
	-	Finish/ Corrosion resistance: To match ironmongery. 
	•	 Holes for components: No larger than required for satisfactory fit/ operation. 
	•	 Adjacent surfaces: Undamaged. 
	•	 Moving parts: Adjusted, lubricated and functioning correctly at completion. 
	860	INSTALLATION OF EMERGENCY EXIT DEVICES
	•	 Standard: Unless specified otherwise, install panic bolts/ latches in accordance with BS EN 
	1125.